# A Tool Used to Conduct Hypsometric Analysis of a Watershed

## Documentation for package ‘hypsoLoop’ version 0.2.0

- DESCRIPTION file.
- User guides, package vignettes and other documentation.

## Help Pages

calc_areas | Function to calculate areas of classes within a categorical raster
check_arguments | Test if user-supplied inputs match the expected arguments type and form
DEM | Digital Elevation Model (DEM) of Yanze Watershed
drawHypsoCurves | Draw Hypsometric curves and calculate hypsometric integrals
generateHypsoTables | Generating hypsometric tables
lulcYanze | Land Use - Land Cover map of Yanze
raster_conversion | Convert the input raster object into terra's SpatRaster object
Vector_conversion | Convert the input vector object into simple features if it's provided as a Spatial object
watersheds | Yanze sub-catchments boundaries
watersheds_df | Yanze sub-catchments table
Yanze_DEM | Digital Elevation Model (DEM) of Yanze Watershed
Yanze_LULC | Land Use - Land Cover map of Yanze
Yanze_sub-catchments | Yanze sub-catchments boundaries
Yanze_sub-catchments-table | Yanze sub-catchments table